S15ABG3-BIOS release note:
R1.08
1. PD power off in S5 when system is in battery
2. Fix disable internal MIC, it will disable handset mic"
3. Add SDD erase in secure page (Sanitization)

R1.07
1. Fix panel flick issue in windows

R1.06
1. Fix system hang-up in windows
2. Add internal speaker/Mic enable/disble in setup menu

R1.05
1. Fix Bitlock fail when enable Secureboot
2. Fix expansionboard disable, it disable 2nd SSD

R1.04
1. Fix panel blinking issue

R1.03
1. Fix DMI data lose if power lose,

R1.02
1. Fix LTE 5G card, 2nd lan fail

R1.01
1. Add fan, MXM fan and KB backlight test
2. Fix HW board version

RC.03: use Adler lake code base
1.Fix "Panel off resime sleep/S4 when LID close
2.Power button changeto fix event for test.
3.EC fix bridge battery switch too long issue.

RC.02: use Adler lake code base
1.Fix TBT fail resume from S4 and plug in TBT monitor
2.do'nt show advance and chipset subpage in setup menu.

RC.01: use Adler lake code base
1.change power on ,PL1/PL2/PL3 = AC mode 68/85/87
2.change PL4=110
3.change DDR ODT disable
4. SA GV 3rd point =4800 G2

RC.00: use Adler lake code base
1.Add EC version in SMBIOS
2.Fix "3 TB device reboot, System hangup"
3.add "setup menu variable function"
4.add DDR ODT 120 ohm
5.add retimer capsule update

RB.07: use Adler lake code base
1.mxm can RTD3 cold
2.fix the function switch the mode serial port,  the 485 mode fail
3.Add secureboot key

RB.06: use Adler lake code base
1.fix mxm cannot enter CPU C8(rB.05 bug)
2.Add the function which change serial port mode by Quick menu
3.Add disable clock request when disable SD car or LTE pcie port.

RB.05: use Adler lake code base
1.change power on ,PL1/PL2/PL3 = AC mode 68/85/87
2.change PL4=107
3.Change PEG port 2, speed=Gen3

RB.04: use Adler lake code base
1. Fix "No blue-tooth issue"
2. Fix "touchpad response issue", which change interrupt from APIC to GPIO.
3. Enable PCIE compliance test mode for some express-cards fail 
4. Fix WWAN/GPS issue
5. Fix Battery information issue, battery capacity  isn't right data
6. Fix Express-card hot-plug fail issue
7. Fix RTC wakeup issue
8. Add CPU throttling function for quick menu

RB.03: use Adler lake code base
1. Fix 5G LTE for modern standby
2. Fix RFID for modern standby
3. Modify battery information for OS in critical low issue of battery
4. BIOS PL1: 28, PL2: 35, PL3:42, PL4: 110
5. DTT Battery:PL1: 28, PL2: 35, PL3:42, AC:PL1: 68, PL2: 85, PL3:87
6. DTT MXM Battery:PL1: 28, PL2: 35, PL3:42, AC:PL1:84, PL2:105, PL3:107
7. Fix SD in enable "ACPI D3 issue" and fail to initiate with 5G or MXM

RB.02: use Adler lake code base
1. Fix MXM clock request issue
2. Fix MXM can enter modern standby

RB.01: use Adler lake code base
1. Load defailt fail
2. add the function for PD firmware
3. fix LID function

RB.00: use Adler lake code base
1. Fix USB type c display cannot display issue
2. Fix TBT cannot display issue
3. Add new DTT for MXM (PL1=90, Pl2=120, Pl3=130),
4. Add Lid function

RA.11: use Adler lake code base
1. fix fsp vga module.

RA.10: use Adler lake code base
1. Update CPU microcode
2. Update new ME code.
3. fix "disable exansion board to disable usb port 9
4. Add detect MXM to EC RAM

RA.09: use Adler lake code base
1. use R11AH7 SSID and driver to fix HDMI audio issue nad sleep issue
2. enable PCIE port 10 hotplug
3. fix TPM disable, load default can not enable
4. PD below 80W, system will warn message during POST
5. Add battery capacity and voltage for battery report

RA.08: use Adler lake code base
1. Expansion board disable, to disable USBHSport[9].
2. If not expresscard, ASPM enable
3. Add Modern Standby,
4. Fix 5G card fail

RA.07A: use Adler lake code base
1. Fix DTT PL1/PL2/PL3 settings
2. Fix Serial port function
3. Change PCIE lane2 (4*1), PCIE port6 disable

RA.06A: use Adler lake code base
1. Fix PCIE aspm
2. Fix expansion board can not power off
3. Add Serial port COM1  function(Brian's machine not work)
4. Add Power DDT function settings(ADC PL1/PL2/PL3=28/35/50, AC PL1/PL2/PL3=80/90/100 

RA.05:
1. Set display mode is HG for MXM
2. Add bridge battery function
3. Fix tbt port display 3 monitor issue
4. Add exoabsion board in setup menu
5. set Expansion board PCIE speed = GEN1
6. Fix battery disapear in windows
7. Add quick menu which read battery status.
8. Add air plaine mode

RA.04:
1. Change PD message during POST
2. Set USB Overcurrent settings
3. Disable D3 cold For fix SD card issue
4. Add SATA port into LED
5. Fix quick menu event from QD8 to QDB.

RA.03:
1. Add clkreq
2. Fix SD card issue
3. Fix battery calibration issue.
4. add Expresscard aspm option

RA.02:
1. No unknown device
2. Camera 沒鏡相問題.
3. All gpio is ok
4. TBT switch pin is exchanged 
