R10-BIOS release note:
R1.00
1. First release for MP

RD.06.
1. low temporary start, fix the marning message
2. Fix diable DMIC when disable internal Mic,
3. Add SSD secure erase function
4. Fix Wifi SAR settings

RD.05
1. Cahnge EC R00.01.15

RD.04
1. Set VDD2H=1060 (origanl 1070, auto)
2. RF request, modify Wifi SAR settings
3. It don't need password to write OA3

RD.03
1. Disable UCSI
2. Fix battery calibration issue
3. Enable BT audio offload.

RD.02
1. Panel brightness table update (RD.01 and Rd.00 fail)
2. enable display port Spread spectrum clock
3. SMBIOS SKU number is set to writable
4. Fix USB Exposed Port System Test(HLK test)
5. Fix USB4 Systems Have Support For All Type-C connectors: t(HLK test) 

RD.01
1. Quick speed from 100KHz to 400KHz
2. Fix usb computer display object tst(HLK)
3.

RD.00
1. Enable Boot guard
2. Enable ME lock
3. Enable Txt
4. Enable secure boot
5. Update microcode to 12.5 

RC.06
1. VGA EFP1 port 1 is set to DP line rate to UHBR20G

RC.05
1. Update MRC code and FSP version for corpoate CPU boot(TAG25-TAG35)

RC.04
1. Add UEFI update function
2. Remove hid event filter device
3. Remove APK sensor from ISH
4. Add Keyboard dock device in asl
5. If no RF switch, remove antenna_switch form
6. Change THC0 SVID/SDID to 0xA05314ff
7. Onekey update to search "Update.nsh"

RC.03
1. modofy battery calibration function
2. SD RTD3 to D3hot
3. Setup menu, BIOS polling CPU temp every 10s

RC.02
1. Change VGA BIOS for panel noise when resume from MS
2. Change EC fw from CPU temp default=40
3. add sensor hub device

RC.01
1. Fix BIOS Version:0.0.0 and CPU Temp=0 power on without power
2. fix press setup icon fail
3. change password rule
4. modify Pd number=1
5. add MElock function
6. Add secureboot app in DB
7. Fxi HLK test for Keyboard, Thermal, USB settings and ISH

RC.00
1. Add Tcc offset=5
2. Add ME-lock update function
3. Modify password complexity 

RB.03
1. Fix MSR and FP enable fail for BIOS RB01
2. Add LID function
3. Add TPM PH randomize
4. disable MeBx hotkey
5. enable edp spread spectrum clock 
6. Add secure flash function

RB.02
1. Fix IrCAM mirror issue
2. Fix setup menu error message
3. Fix Quick menu fail

RB.01,
1. ESPI set to Qual mode
2. fix SD card initial and UnMute issue
3. Fix Touch panel and disable THC1
4. Fix RB.00 audio unknown device

RA.11
1. modify usb type C function of setup menu 
2. Add P button and modify P2 button functions of setup menu 
3. Fix SD card disappears in Win11 sometimes.
4. Add B_17 for retimer power
5. Add Digitizer enable/disable

RA.10
1. fix quick menu fail issue
2. Add Virtual Keyboard and setup menu and Boot manager buttons during POST
3. enable Secure flash function

RA.09
1. Add warning message during POST, in temperature -29
2. Add EC and HW version to SMBIOS
3. Modify BIOS version in SMBIOS
4. Change espi mode from qual mode to dual mode
5. Change UUID display format in setup menu

RA.08
1. Add popup message for PD power < 60W
2. Add Pluton device
3. Add secure boot item
4. Add VTIO for IRCAM
5. Change PME wake to RTC wake

RA.07
1. change ACPI settings for better power consumption in sleep
2. add BIOS show the second of RTC, and show CPU Temperature
3. add numlock of Boot sub menu
4. Change onekey flash for search "Update.nsh" file

RA.06
1. Change Brightness table
2. add power button to shut down during setup menu
3. disable THC0 GPIO for modern standby
4. Fix SD card disable, re-enable, SD card will disappear
5. Panel power on brightness = 20%
6. Add Onekey flash function
7. Fix TBT connect 2 monitors issue
8. Add touch panel function on setup menu

RA.05
1. Add Pluton function
2. Disable clock request when PCIE port disable
3. add brightness table 
4. Add ECNT method for sleep , system will turn off power led 
5. disable wireless configure device

RA.04
1. Fix USB Type A 3.0 fail to disable and USB 2.0 issue
2. Fix BT speaker issue
3. Fix touchscreen mode 
4. Add quick menu, Q-event 0xdc and barcode event
5. fix RF switch issue
6. Fix resume from S4, Q event fail

RA.03
1. Add USB type A port enable/disable
2. Add USB Type C
3. Add Touch screen mode and enable/disable
4. Add THC0 dummy driver
5. disable DPTF
6. fix USB/Serial port/expansion board enable/disable

RA.02:
1. Add Camera mirror issue
2. modify advance of setup, it overwrite data to nvram
3. Add Sensor hub data
4. set SD-card reader D3 hot
5. Set vc1/vc2//vc3 for quick menu
6. Set TS mode for quick menu

RA.01:
1. Setup menu device enable/disable settings are ok.
2. Serial port mode is ok
3. Add Psys max, PL1/2/3/4
4. 5G reset is ok
5. disable IPU
6. disable I2C0,ISH-I3C1 ISH-I2c2 “USB PDO programming”


